For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 29792 Lower Control Arm Front Bushing Set

• | J 41211 Lower Control Arm Vertical Bushings

1. Remove the lower control arm. Refer to Lower Control Arm Replacement Lower Control Arm Replacement .
2. Install the bushing removal tools (1, 3, 5).
3. Coat threads of the bolt (1) with an extreme pressure lubricant.
4. Remove the lower control arm bushings (4).
5. Remove the lower control arm vertical bushing (3).

### Installation Procedure

1. Install the bushing installation tools (1, 3, 5).
2. Install the front control arm bushing (2).
3. Install the rear control arm vertical bushing (2).
4. Lubricate the outer casing of the new bushing (2).
5. Install the lower control arm bushings (2).
6. Install the lower control arm (4). Refer to Lower Control Arm Replacement