For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Seats System Check? | -- | Go to Step 2 | Go to Power Seats System Check
2 |

1. Disconnect the seat switch connector.
2. Connect a test lamp between terminal F and ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 |

1. Ensure that the seat switch connector is still disconnected.
2. Connect a test lamp between terminal F and terminal C.

Does the test lamp light?

--

Go to Step 5

Go to Step 6

4 | Repair the open in CKT 60 or CKT 540. Is the repair complete? | -- | Go to Power Seats System Check | --
5 |

1. Ensure that the seat switch was mated correctly.
2. If OK, replace the seat switch.

Refer to Front Seat Adjuster Motor Replacement .

Is the repair complete?

--

Go to Power Seats System Check

--

6 | Repair the open in CKT 150. Is the repair complete? | -- | Go to Power Seats System Check | --