For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Bearing and Shim Retainer Screws | 23 N·m | 17 lb ft
Control Box to Case Bolts | 17 N·m | 13 lb ft
Detent Spring Retaining Bolts | 25 N·m | 18 lb ft
Input/Output Shaft Retaining Nuts | 128 N·m | 94 lb ft
Rear Cover Bolts | 17 N·m | 13 lb ft
Reverse Idle Shaft Bolt | 38 N·m | 28 lb ft
Reverse Shift Bracket Retaining Bolts | 17 N·m | 13 lb ft
Transaxle Case To Clutch Housing Bolts | 38 N·m | 28 lb ft
Backup Light Switch | 33 N·m | 24 lb ft
Clutch Housing Cover Bolt | 10 N·m | 89 lb in
Shift Cable Cover Bolt | 1.4 N·m | 12 lb in
Shift Control Box Bolt | 17 N·m | 13 lb ft
Shift Control Box Nut | 24 N·m | 18 lb ft
Shift Linkage Retainer Nut | 23 N·m | 17 lb ft
Shift Retainer Nut | 10 N·m | 89 lb in
Speedometer/Vehicle Speed Sensor Housing Bolt | 9 N·m | 80 lb in
Transaxle-to-Engine Mounting Bolts and Stud | 90 N·m | 66 lb ft
Transaxle Mount Bolt | 75 N·m | 55 lb ft
Transaxle Mount Through Bolt | 60 N·m | 44 lb ft
Transaxle Shift Cable Bracket Nut | 10 N·m | 89 lb in
Transaxle Shift Lever Nut | 10 N·m | 89 lb in

Application | Specification
--- | ---
Metric | English
Backup LIght Switch | 33 N·m | 24 lb ft
Clutch Housing Cover Botl | 10 N·m | 89 lb in
Shift Cable Cover Bolt | 1.4 N·m | 12 lb in
Shift Control Box bolt | 17 N·m | 13 lb ft
Shift Control Box Nut | 24 N·m | 18 lb ft
Shift Linkage Retainer Nut | 23 N·m | 17 lb ft
Shift Retainer Nut | 10 N·m | 89 lb in
Speedometer/Vehicle Speed Sensor Housing Bolt | 9 N·m | 80 lb in
Transaxle-to-Engine Mounting Bolts and Stud | 90 N·m | 66 lb ft
Transaxle Mount Bolt | 75 N·m | 55 lb ft
Transaxle Mount Through Bolt | 60 N·m | 44 lb ft
Transaxle Shift Cable Bracket Nut | 10 N·m | 89 lb ft
Transaxle Shift Lever Nut | 10 N·m | 89 lb ft