For 1990-2009 cars

# June 1999 Labor Time Guide Updates

Subject: | June, 1999 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PANEL, FRONT DOOR TRIM FINISH UPPER FRONT - R&R OR REPLACE

- PART GP: 10.485

RIGHT |  | C3330 | -- | -- | -- | 0.4 | 0.4 | 0.4 | 0.4
LEFT |  | C3331 | -- | -- | -- | 0.4 | 0.4 | 0.4 | 0.4
ADD:

- A- To Color/Clear Coat

N

--

--

--

0.4

GD

0.4

GD

0.4

GD

0.4

GD

*IND: N - New/R - Revised

#### LTG Update - C/K Platform - New Body Style

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
ADJUSTER ASSEMBLY, FRONT SEAT MANUAL - R&R OR REPLACE

- PART GP: 11.561

BENCH SEAT |  | C6000 |  |  |  |  |  |  |
ONE SIDE |  |  | -- | -- | -- | -- | -- | 0.5 | 0.5
BUCKET SEAT |  |  |  |  |  |  |  |  |
PASSENGER |  | C6010 |  |  |  |  |  |  |
ONE SIDE | R |  | -- | -- | -- | -- | -- | 0.8 | 0.8
BUCKET SEAT |  |  |  |  |  |  |  |  |
DRIVER |  | C6011 |  |  |  |  |  |  |
ONE SIDE | R |  | -- | -- | -- | -- | -- | 0.8 | 0.8
SPLIT/DIVIDED SEAT |  |  |  |  |  |  |  |  |
PASSENGER |  | C6020 |  |  |  |  |  |  |
ONE SIDE |  |  | -- | -- | -- | -- | -- | 0.6 | 0.6
SPLIT/DIVIDED SEAT |  |  |  |  |  |  |  |  |
DRIVER |  | C6021 |  |  |  |  |  |  |
ONE SIDE |  |  | -- | -- | -- | -- | -- | 0.6 | 0.6
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
PUMP, ENGINE OIL - REPLACE

- PART GP: 1.652

- NOTE: Applies to Engine Code V, T, U

J1020

C TRUCK |  |  | -- | -- | -- | -- | -- | 3.2 | 3.2
K TRUCK | R |  | -- | -- | -- | -- | -- | 4.1 | 4.1
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
HOUSING AND/OR GASKET, REAR MAIN SEAL - REPLACE

- No Change to "PART GP" or "INC"

- NOTE: Applies to Engine Code V, T, U

J1080

MANUAL TRANS |  |  |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 3.3 | 3.3
K TRUCK |  |  | -- | -- | -- | -- | -- | 4.1 | 4.1
AUTO TRANS |  |  |  |  |  |  |  |  |
C TRUCK |  |  | -- | -- | -- | -- | -- | 3.5 | 3.5
K TRUCK | R |  | -- | -- | -- | -- | -- | 5.5 | 5.5
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
PROM - REPROGRAMMING

- POLICY: E

ON CAR | R | J6355 | -- | -- | -- | -- | -- | 0.5 | 0.5
TRANSMISSION ASSEMBLY - REPLACE

- No Change to "PART GP," "INCs," or "NOTEs"

- NOTE: Applies to 4L80E

K7000

C TRUCK |  |  | -- | -- | -- | -- | -- | 3.7 | 3.7
K TRUCK | R |  | -- | -- | -- | -- | -- | 5.8 | 5.8
ADD:

- A- W/Skid Plate

R

--

--

--

--

--

0.1

0.1

B- To Replace Flywheel |  |  | -- | -- | -- | -- | -- | 0.2 | 0.2
C- To Disassemble, Inspect And Reassemble Core Transmission/Transaxle (0.0-1.5) | N |  | -- | -- | -- | -- | -- | 0-1.5 | 0-1.5
CONVERTER ASSEMBLY, TRANSMISSION - REPLACE

- No Change to "PART GP," "INCs," or "NOTE"

- NOTE: Applies to 4L80E

K7020

C TRUCK |  |  | -- | -- | -- | -- | -- | 3.9 | 3.9
K TRUCK | R |  | -- | -- | -- | -- | -- | 5.1 | 5.1
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
TRANSMISSION ASSEMBLY - REPLACE

- No Change to "PART GP," "INC," or "NOTE

- NOTE: Applies to 4L60E

K7000

C TRUCK | R |  | -- | -- | -- | -- | -- | 3.9 | 3.9
K TRUCK | R |  | -- | -- | -- | -- | -- | 5.6 | 5.6
ADD:

- A- W/Skid Plate

--

--

--

--

--

0.2

0.2

B- To Replace Flywheel |  |  | -- | -- | -- | -- | -- | 0.2 | 0.2
C- To Disassemble, Inspect And Reassemble Core Transmission/Transaxle (0.0-1.5) | N |  | -- | -- | -- | -- | -- | 0-1.5 | 0-1.5
CONVERTER ASSEMBLY, TRANSMISSION - REPLACE

- No Change to "PART GP" or "INCs"

- NOTE: Applies to 4L60E

K7020

C TRUCK |  |  | -- | -- | -- | -- | -- | 3.7 | 3.7
K TRUCK | R |  | -- | -- | -- | -- | -- | 4.9 | 4.9
ADD:

- A- W/Skid Plate

--

--

--

--

--

0.2

0.2

B- To Recondition Trans Completely | R |  | -- | -- | -- | -- | -- | 5.7 | 5.7
C- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec |  |  | -- | -- | -- | -- | -- | 0.5 | 0.5
*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MANIFOLD AND/OR GASKET, INTAKE - REPLACE

- No Change to "PART GP," "POLICY," or "NOTE"

- NOTE: Applies to Engine Code C

J0200

--

1.4

1.4

1.4

1.4

1.4

ADD:

- A- To Replace Intake Manifold

N

--

0-.2

0-.2

0-.2

0-.2

0-.2

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
CUP HOLDER, CONSOLE - REPLACE

- PART GP: 10.240

FRONT AND/OR REAR |  | C2745 |  |  |  |  |  |  |
PONTIAC/BUICK | R |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
OLDSMOBILE |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.3 | 0.3 |
*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PISTON, ROD AND/OR RINGS - REPLACE

- No Change to "PART GP" or "INC"

- NOTE: Applies to Engine Code M and E

ONE CYL |  |  |  |  |  |  |  |  |
RIGHT BANK |  | J1300 |  |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | -- | -- | 6.1 | 6.1 | 6.1 | 6.1
GRAND AM, ACHIEVA, SKYLARK & ALERO | R |  | 10.6 | 10.6 | 10.6 | 10.6 | 10.6 | 10.6 | 10.6
ONE CYL |  |  |  |  |  |  |  |  |
LEFT BANK |  | J1301 |  |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | -- | -- | 5.8 | 5.8 | 5.8 | 5.8
GRAND AM, ACHIEVA, SKYLARK & ALERO | R |  | 9.0 | 9.0 | 9.0 | 9.0 | 9.0 | 9.0 | 9.0
ONE CYL |  |  |  |  |  |  |  |  |
BOTH BANKS |  | J1307 |  |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | -- | -- | 7.4 | 7.4 | 7.4 | 7.4
GRAND AM, ACHIEVA, SKYLARK & ALERO | R |  | 12.4 | 12.4 | 12.4 | 12.4 | 12.4 | 12.4 | 12.4
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - P/H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
MODULE, ELECTRONIC THROTTLE CONTROL - REPLACE | N | J5582 | -- | -- | -- | -- | 0.6 | 0.6 |
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PUMP, SECONDARY AIR INJECTION - REPLACE | N | J6050 | -- | -- | -- | -- | 0.7 | 0.7 | 0.7
*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
ROD ASSY, REAR AXLE TIE - R&R OR REPLACE | R | E4200 | 0.5 | 0.5 | 0.5 | 0.3 | 0.3 | 0.3 | 0.3
*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
CARPET, FLOOR - R&R OR REPLACE

- PART GP: 15.286

- POLICY: S Additional .3 hours if the vehicle is delivered to and from the repair location.

ONE PIECE | R | C4208 |  |  |  |  |  |  |
4 DOOR |  |  |  |  |  |  |  |  |
CHEVROLET |  |  | 2.0 | 2.0 | 2.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC/BUICK |  |  | 2.0 | 2.0 | 2.0 | 1.0 | 1.0 | 1.0 | 1.0
OLDSMOBILE |  |  | 2.0 | 2.0 | 2.0 | 2.0 | 1.0 | 1.0 | 1.0
2 DOOR |  |  |  |  |  |  |  |  |
CHEVROLET |  |  | 2.0 | 2.0 | 2.0 | 1.0 | 1.0 | 1.0 | 1.0
PONTIAC |  |  | 2.0 | 2.0 | 2.0 | 1.0 | 1.0 | 1.0 | 1.0
ADD:

- A- W/Console

Chevrolet |  |  | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
Pontiac/Buick |  |  | 0.4 | 0.4 | 0.4 | 0.3 | 0.3 | 0.3 | 0.3
Oldsmobile |  |  | 0.4 | 0.4 | 0.4 | 0.4 | 0.3 | 0.3 | 0.3
PAN AND/OR GASKET, OIL - REPLACE

- No Change to "PART GP" or "NOTE"

- NOTE: Applies to Engine Code M and T

R

J1000

CHEVROLET |  |  | 3.5 | 3.5 | 2.5 | 2.5 | 2.5 | 2.5 | 2.5
PONTIAC |  |  | 3.5 | 3.5 | 3.5 | 2.3 | 2.3 | 2.3 | 2.3
OLDSMOBILE |  |  | 3.5 | 3.5 | 3.5 | 3.5 |  |  |
BUICK |  |  | 3.5 | 3.5 | 3.5 | 2.3 | 2.3 | 2.3 | 2.3
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
PASSIVE KEYLESS ENTRY (PKE) SYSTEM COMPONENTS - REPLACE

- INC: Reprogramming

TRANSMITTER |  | R3011 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
MODULE | R | R3012 |  |  |  |  |  |  |
COUPE |  |  | 1.1 | 1.1 | 1.1 | 0.6 | 0.6 | 0.6 | 0.6
CONVERTIBLE |  |  | 1.1 | 1.1 | 1.1 | 0.3 | 0.3 | 0.3 | 0.3
BATTERY |  | R3013 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
RECEIVER ANTENNA |  |  |  |  |  |  |  |  |
DRIVER DOOR |  | R3014 | 1.1 | 1.1 | 1.1 |  |  |  |
PASSENGER DOOR |  | R3016 | 1.1 | 1.1 | 1.1 |  |  |  |
REAR LIFT WINDOW |  | R3019 | 0.4 | 0.4 | 0.4 | 0.2 | 0.2 | 0.2 | 0.2
No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised