For 1990-2009 cars

## Air Conditioning Compressor Bracket Replacement 2.4L

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the belt. Refer to Drive Belt Replacement in Engine Mechanical - 2.4L.
3. Remove the generator. Refer to Generator Replacement in Engine Electrical.
4. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
5. Remove the compressor attaching bolts (1,2,3,5).
6. Remove the compressor (4). Refer to Air Conditioning Compressor Replacement .
7. Remove the bracket.

### Installation Procedure

Important: Repairs to the following areas require the loosening of some A/C bracket bolts:

• | The A/C compressor

• | The A/C belt system

In order to prevent future torque loss after retightening the bolts, perform the following steps:

• | Replace the bolt with an appropriate new bolt.

• | Replace the stud with an appropriate new stud.

• | Apply Loctite® 242 or the equivalent to the bolt or stud threads.

| Follow the package instructions in order to achieve the best retention.

1. Install the bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the following components:

• | The compressor (4)

• | Refer to Air Conditioning Compressor Replacement .

• | The compressor attaching bolts (1,2,3,5)

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Lower the vehicle.
4. Install the generator. Refer to Generator Replacement in Engine Electrical.
5. Install the drive belt. Refer to Drive Belt Replacement in Engine Mechanical - 2.4L.
6. Connect the negative battery cable.

Tighten
Tighten the bolt to 16 N·m (12 lb ft).

## Air Conditioning Compressor Bracket Replacement 3.1L

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the drive belt. Refer to Drive Belt Replacement in Engine Mechanical - 3.1L.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
4. Remove the splash shield. Refer to Splash Shield Replacement - Wheelhouse in Body Front End.
5. Remove the compressor attaching bolts (1).
6. Remove the compressor (2). Refer to Air Conditioning Compressor Replacement .
7. Remove the spacer (3).

### Installation Procedure

Important: Repairs to the following areas require the loosening of some A/C bracket bolts:

• | The A/C compressor

• | The drive belt system

In order to prevent future torque loss after retightening the bolts, perform the following steps:

• | Replace the bolts with an appropriate new bolt.

• | Apply Loctite® 242 or the equivalent to the bolt or stud threads.

| Follow the package instructions in order to achieve the best retention.

1. Install the spacer (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the following components:

• | The compressor (2)

• | Refer to Air Conditioning Compressor Replacement .

• | The compressor attaching bolts (1)

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Install the splash shield. Refer Splash Shield Replacement - Wheelhouse in Body Front End.
4. Lower the vehicle.
5. Install the drive belt. Refer to Drive Belt Replacement in Engine Mechanical - 3.1L.
6. Connect the negative battery cable.

Tighten
Tighten the bolt to 16 N·m (12 lb ft).