For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel. Refer to Instrument Panel Replacement .
2. Disconnect the wiring harness from the tie bar.

Remove the bolts from the tie bar.

3. Remove the tie bar from the front of the dash.

### Installation Procedure

1. Install the tie bar to the front of the dash.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts and the studs to the tie bar.

Tighten
Tighten the bolts and the studs to 10 N·m (89 lb in).

3. Connect the wiring harness to the tie bar.
4. Install the instrument panel. Refer to Instrument Panel Replacement .