For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 28467-360 Engine Support Fixture

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Install the J 28467-360 to the transmission.
3. Remove the upper transmission mount assembly bolts.
4. Raise the vehicle. Support the vehicle. Refer to Vehicle Lifting Caution in General Information.
5. Remove the left front tire and the wheel assembly. Refer to Wheel Removal in Tires and Wheels.
6. Remove the left front splash shield.
7. Remove the transmission mount expansion pipe bolt.
8. Remove the lower transmission mount assembly bolts.
9. Remove the transmission mount.

### Installation Procedure

1. Install the transmission mount.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the upper transmission mount bolts.

Tighten
Tighten the bolts to 66 N·m (49 lb ft).

3. Install the transmission mount expansion plug.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

4. Install the left front splash shield.
5. Install the left front tire and the wheel assembly. Refer to Wheel Installation in Tires and Wheels.
6. Lower the vehicle.
7. Install the lower transmission mount bolts.

Tighten
Tighten the bolts to 66 N·m (49 lb ft).

8. Remove the engine support fixture.
9. Connect the negative battery cable.