For 1990-2009 cars

Important: Handle the vehicle speed sensor assembly carefully.

1. Inspect the vehicle speed sensor assembly (10) and the vehicle speed sensor O-ring seal (11) for the following conditions:

• | Damaged connector

• | Cracked housing

• | Signs of rotor damage

• | Cuts or nicks on the O-ring seal

2. Install a new O-ring seal (11) on the vehicle speed sensor assembly (10).
3. Install the vehicle speed sensor assembly (10) into the case extension.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the vehicle speed sensor bolt (9).

Tighten
Tighten the bolt to 12 N·m (106 lb in).