For 1990-2009 cars

#### Tools Required

• | J 23738-A Hand Vacuum Pump (or equivalent)

• | J 36619 Modulator Checking Tool

1. Inspect the modulator components for the follow conditions:

• | A damaged modulator valve (34)

• | A damaged modulator assembly (32)

• | A damaged modulator O-ring seal (33)

• | A damaged modulator retainer (31)

2. Install J 23738-A or equivalent onto the vacuum pipe nipple of the modulator assembly.
3. Apply 15 kPa of vacuum to the modulator assembly (32) under the following criteria:

• | Hold the vacuum for 30 seconds

• | Confirm that the plunger retracts into the modulator assembly

4. Remove J 23738-A from the modulator assembly.
5. Use a modulator assembly that is known to be good.
6. Install J 36619 between the good modulator and the modulator to be checked.
7. Push the modulators towards each other.
8. Note the indicator on J 36619 :

• | If the indicator line (1) is visible, the modulator is OK

• | If the indicator line moves out of view, replace the modulator