For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 25034-C Power Steering Pump Pulley Remover

• | J 25033-C Power Steering Pump Pulley Installer

1. Remove the belt from the pulley.
2. Remove the pump from the engine for tool clearance. Refer to Power Steering Pump Replacement .

You are not required to remove the pressure lines or the return lines from the pump.

3. Use the J 25034-C in order to remove the pulley.

### Installation Procedure

Important:

• | The face of the pulley hub must be flush with the pump drive shaft.

• | Do not use the arbor press in order to install the pulley.

1. Install the power steering pump pulley using the J 25033-C .
2. Install the pump to the engine. Refer to Power Steering Pump Replacement .
3. Install the belt on the pulley.
4. If the pump was removed from the engine, bleed the power steering system. Refer to Power Steering System Bleeding .