For 1990-2009 cars

## Outside Rearview Mirror Replacement Manual

### Removal Procedure

1. Remove the door rear view mirror bezel screw.
2. Remove the door rear view mirror bezel.
3. Remove remote control from the bezel.
4. Remove the insulator (1).
5. Remove the rear view mirror nuts (3).
6. Remove the rear view mirror (4).

### Installation Procedure

1. Install the rear view mirror (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear view mirror nuts (3).

Tighten
Tighten the nut to 5.6 N·m (50 lb in).

3. Install the insulator (1).
4. Install remote control from the bezel.
5. Install the door rear view mirror bezel.
6. Install the door rear view mirror bezel screw.

Tighten
Tighten the screw to 1 N·m (9 lb in).

## Outside Rearview Mirror Replacement Power

### Removal Procedure

1. Remove the door rear view mirror bezel screw.
2. Remove the door rear view mirror bezel.
3. Remove power mirror wire harness (2).
4. Remove the insulator (1).
5. Remove the rear view mirror nuts (3).
6. Remove the rear view mirror (4).

### Installation Procedure

1. Install the rear view mirror (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear view mirror nuts (3).

Tighten
Tighten the nut to 5.6 N·m (50 lb in).

3. Install the insulator (1).
4. Install the power mirror wire harness (2).
5. Install the door rear view mirror bezel.
6. Install the door rear view mirror bezel screw.

Tighten
Tighten the screw to 1 N·m (9 lb in).