For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Coolant Outlet Assembly Bolts 2.4L (4 cyl.) | 26 N·m | 19 lb ft
Fan Assembly Motor to Fan | 3.3 N·m | 29 lb in
Fan-to-Radiator Support Bolt | 11 N·m | 97 lb in
Radiator Outlet Pipe to Water Pump Cover 2.4L (4 cyl.) | 14 N·m | 124 lb in
Radiator Outlet Pipe to Engine Oil Pan 2.4L (4 cyl.) | 25 N·m | 18 lb ft
Radiator Surge Tank Inlet Pipe Fitting 3.1L (6 cyl.) | 21 N·m | 15 lb ft
Radiator to Radiator Support Bolts | 10 N·m | 89 lb in
Surge Tank Bolts | 9 N·m | 80 lb in
Surge Tank Cap | 4 N·m | 35 lb in
Surge Tank Inlet Pipe to Block Fitting 3.1L (6 cyl.) | 21 N·m | 15 lb ft
Transaxle Oil Cooler Pipe Fittings at Radiator | 30 N·m | 22 lb ft
Water Pump Cover to Block Bolts 2.4L (4 cyl.) | 26 N·m | 19 lb ft
Water Pump Pulley to Pump Bolts 3.1L (6 cyl.) | 25 N·m | 18 lb ft
Water Pump to Water Pump Cover Bolts 2.4L (4 cyl.) | 14 N·m | 124 lb in
Water Pump to Front Cover Bolts 3.1L (6 cyl.) | 10 N·m | 89 lb in
Water Pump to Timing Chain Housing 2.4L (4 cyl.) | 26 N·m | 19 lb ft