For 1990-2009 cars

### Removal Procedure

1. Remove the left sound insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges, and Console.
2. Disconnect the turn/hazard flasher connector.
3. Remove the turn/hazard connector.

### Installation Procedure

1. Install the turn/hazard flasher.
2. Connect the turn/hard flasher connector.
3. Install the left sound insulator. Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges, and Console.