For 1990-2009 cars

# LOOSE MIRROR REMOTE ASSY. REPL. FRT SIDE UPPER DOOR TRIM

#### SUBJECT: LOOSE MIRROR REMOTE CONTROL ASSEMBLY (REPLACE FRONT SIDE UPPER DOOR TRIM)

#### VEHICLES AFFECTED: 1992 "N" MODELS

#### CONDITION:

--------- Some owners of 1992 "N" cars may comment that the left hand mirror cable remote control assembly becomes loose at the front side upper door trim.

#### CAUSE:

----- Inadequate retention of the set screw to the palnut.

#### CORRECTION:

---------- Replace the existing front side upper door trim with the appropriate revised part listed below:

Pontiac/Oldsmobile Panel, assembly-front side door upper front trim finish ------------------ ------------------------------- P/N 22587635 Graphite P/N 22587636 Camel P/N 22587637 Medium Gray P/N 22587638 Garnet

#### Buick

P/N 22587643 Medium Gray P/N 22587644 Graphite P/N 22587645 Camel P/N 22587646 Garnet

For vehicles repaired under warranty use:

Labour Time: 0.2 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.