For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the fluid level switch (1).
2. Disconnect the fluid level switch (1) using needle nose pliers in order to compress the switch locking tabs (1) at the inboard side of the master cylinder reservoir (2).

### Installation Procedure

1. Connect the fluid level switch (1) into the master cylinder reservoir until the locking tabs (3) snap into place.
2. Connect the electrical connector to the fluid level switch (1).