For 1990-2009 cars

#### Tools Required

• | J 8092 Driver Handle

• | J 33833 Bearing Installer

• | J 33833 Bearing Installer

• | J 33843 Seal Installer

• | J 33831 Seal Installer

• | J 33832 Bearing Installer

1. Install the following components into the front case half:

1.1. | The detent plunger

1.2. | The detent spring

1.3. | The O-ring seal

1.4. | The detent plug

Tighten
Tighten the detent plug to housing to 15 N·m (11 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the vehicle speed sensor and the O-ring to the rear housing.

Tighten
Tighten the vehicle speed sensor to 31 N·m (23 lb ft).

3. Install the vacuum switch and the O-ring to the front case housing.

Tighten
Tighten the vacuum switch to 24 N·m (17 lb ft).

Important: Use Dexron® III automatic transmission fluid or the equivalent for lubricant during assembly.

4. Use the J 33832 and the J 8092 to install the needle bearings into the rear case half.

Make sure that the bearing is flush with the boss on the case housing.

5. Use the J 8092 and the J 33833 to install the front output bearing into the front case half.
6. Install the front output bearing snap ring.
7. Use the J 33833 and the J 8092 to install the bearing into the rear retainer housing.
8. Use the J 33833 and the J 8092 to install the bearing into the input gear.
9. Install the thrust washer into the planetary carrier.
10. Install the input gear and the thrust washer into the planetary carrier.
11. Install the input gear to the planetary carrier snap ring.
12. Use the J 33833 to install the bearing into the front case half.
13. Use the J 33843 to install the oil seal into the rear extension.
14. Use the J 33831 to install the input bearing retainer seal into the input bearing retainer.
15. Use the J 33843 to install the front output shaft seal into the front case half.
16. Install the magnet into the front case half.