For 1990-2009 cars

### Removal Procedure

1. Remove the wire harness connector from the clutch pedal position switch.
2. Remove the clutch pedal position switch from the clutch pedal assembly.

### Installation Procedure

1. Install the clutch pedal position switch to the clutch pedal assembly.
2. Install the wire harness connector to the clutch pedal position switch.
3. Verify proper operation of the clutch pedal position switch. The starter should engage only when the clutch is fully disengaged.