For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Low clutch pedal or pedal on the floor.
1 | Inspect the clutch release bearing for binding. Is there binding on the clutch release bearing? | -- | Go to Step 2 | Go to Step 3
2 | Lubricate and free-up the clutch release bearing or replace the clutch actuator. Refer to Clutch Actuator Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | -- | Go to Step 3 | System OK
3 | Check to see if the master cylinder pushrod has fallen off the clutch pedal. Has the master cylinder pushrod fallen off the clutch pedal? | -- | Go to Sep 4 | Go to Step 5
4 | Correctly install the master cylinder pushrod. Refer to Master Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | -- | Go to Step 5 | System OK
5 | Check the hydraulic hose for a hole or leaks. Is the hose OK? | -- | System OK | Go to Step 6
6 | Replace the hydraulic hose. Refer to Master Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | -- | Go to Step 7 | System OK
7 | Check the hydraulic fluid in the reservoir. Is the reservoir full? | -- | System OK | Go to Step 8
8 | Fill the reservoir with fluid. Does the clutch pedal still stay on the floor when disengaged? | -- | Go to Step 9 | System OK
9 | Inspect the master cylinder seal and the master cylinder center valve seal. Is the master cylinder seal or the master cylinder center valve seal faulty? | -- | Go the Step 10 | --
10 | Replace the master cylinder. Refer to Master Cylinder Replacement . Does the clutch pedal still stay on the floor when disengaged? | -- | -- | System OK