For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Gears are clashing and/or grinding in all speeds
1 | Inspect the transaxle fluid level. Refer to Transmission Fluid Check Fill as necessary. Do the gears still grind or clash? |  | Go to Step 2 | System OK
2 |

1. Check the clutch spin down time. Refer to Clutch Spin Down Time
2. Adjust as necessary.

Do the gears still grind or clash?

Go to Step 3

System OK

3 | Check the clutch master cylinder reservoir fluid level. Refer to Hydraulic Clutch Fluid in Clutch. Fill as necessary. Do the gears still grind or clash? |  | Go to Step 4 | System OK
4 |

1. Check the following components for signs of excessive wear or bluing of metal. Some wear is normal.

• | The blocker ring

• | The blocker cone

2. Adjust, repair, or replace components as necessary.

Do the gears still grind or clash?

Refer to Isolating Noise

System OK