For 1990-2009 cars

## Air Filter Element and Air Cleaner Assembly Air Filter Element/Air Cleaner

### Removal Procedure

1. Remove the air cleaner assembly cover.
2. Remove the air filter element.
3. Inspect the air filter element for dust, dirt, water and replace if required. Refer to General Information.

### Installation Procedure

1. Install the air filter element.
2. Install air cleaner cover assembly.
3. Lower Air Cleaner

## Air Filter Element and Air Cleaner Assembly Front Air Intake Duct

### Removal Procedure

1. Remove the front air intake duct.
2. Remove the attaching bolt from the lower air cleaner.
3. Loosen clamp on rear air intake duct and position rear air intake duct aside.
4. Remove lower air cleaner.

### Installation Procedure

1. Install lower Air Cleaner to vehicle.
2. Ensure that the engaging pins are properly located and intake duct is sealed to the intake resonator and front intake duct.
3. Position rear intake duct onto lower air cleaner.
4. Install attaching bolt to lower air cleaner.
5. Install front air intake duct push pin.

## Air Filter Element and Air Cleaner Assembly Air Intake Resonator

### Removal Procedure

1. Remove the attaching bolt.
2. Remove retainer from resonator.
3. Remove the air intake resonator.

### Installation Procedure

1. Install resonator to vehicle.
2. Connect retainer to the air intake resonator.
3. Install attaching bolt to the resonator.