For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief .
2. Drain the fuel tank. Refer to Fuel Tank Draining Procedure .
3. Remove the fuel tank. Refer to Fuel Tank Replacement .
4. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
5. Note the strainer (1) position for future reference.
6. Support the reservoir with one hand and grasp the strainer with the other hand.
7. Use a screwdriver to pry the strainer ferrule off the reservoir.
8. Discard the strainer.

### Installation Procedure

1. Support the reservoir with one hand and grasp the strainer (1) with the other hand twisting the strainer into position.
2. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
3. Install the fuel tank. Refer to Fuel Tank Replacement .
4. Refill tank.
5. Install the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   .
6. Inspect for fuel leaks through the following steps:

6.1. | Turn the ignition switch to the ON position for two seconds.

6.2. | Turn the ignition switch OFF position for ten seconds.

6.3. | Turn the ignition switch to the ON position.

6.4. | Check for fuel leaks.