For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Information.
2. Remove the transmission oil cooler lines from the radiator.
3. Remove the transmission oil cooler lines from the transmission.

### Installation Procedure

1. Install the transmission oil cooler lines to the transmission.

Tighten
Tighten the pipe fitting 32 to 44 N·m (24 to 33 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the transmission oil cooler lines to the radiator.