For 1990-2009 cars

# SMU - SECTION 6E3 - DRIVEABILITY & EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E3-DRIVEABILITY AND EMISSIONS- REVISED PCM CONNECTOR "A" END VIEW

#### MODELS: 1995 PONTIAC GRAND AM 1995 OLDSMOBILE ACHIEVA 1995 BUICK SKYLARK WITH 3.1L ENGINE (VIN M - RPO L82)

ON PAGE 6E3-A-10 AND 6E3-A-11, THE PCM "B" BLACK CONNECTOR IS REPEATED. THE PCM "A" CLEAR CONNECTOR SHOULD BE PLACED ON PAGE 6E3-A-10.

PLEASE MAKE CHANGES IN THE APPROPRIATE 1995 SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 01

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.