For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Remove the LF tire and wheel.
3. Remove the LF wheel house panel.
4. Remove the resonator lower attaching bolt.
5. Remove the resonator attaching fastener.
6. Remove the resonator assembly through wheel house opening.

### Installation Procedure

1. Install the resonator assembly through the wheel house opening.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Verify the full engagement of the resonator to the air intake duct.

2. Install the resonator attaching fastener and the lower attaching bolt.

Tighten
Resonator attaching bolt to 6 N·m (53 lb in).

3. Install the LF wheel house panel.
4. Install the LF tire and wheel.
5. Lower the vehicle.