For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and the wheel. Refer to Wheel Removal in Tires and Wheels.
3. Remove the screws (2) from the wheel housing.
4. Remove the bolts (3) from the wheel housing.
5. Remove the wheel housing (1).

### Installation Procedure

1. Install the wheel housing (1).
2. Install the bolts (3) to the wheel housing.
3. Install the screws (2) to the wheel housing.
4. Install the tire and the wheel. Refer to Wheel Installation in Tires and Wheels.
5. Lower the vehicle.