For 1990-2009 cars

# CREAK CONDITION, FRT. SEATS INSTALL NEW SPACER

#### SUBJECT: BUCKET FRONT SEAT CREAK CONDITION DUE TO SPACE BETWEEN PIVOT PIN AND BUSHING - INSTALL SPACER

#### MODEL/YEARS 1992 ACHIEVA W/AR9 OPTION

CONDITION: Some owners of 1992 Achieva models with AR9 front bucket seats may comment that when making a sharp right or left turn, a creaking noise from the driver seat, and front passenger seat (when occupied) may occur.

CAUSE: Excessive space between the inner front seatback pivot pin and the pivot bushing.

#### CORRECTION:

---------- 1. Put seatback in its most forward position.

2. From rear of seat, install spacer P/N 16743252 on pivot pin. This part is currently available from GMSPO.

Labor Operation: C6520 and C6521

Labor Time: 0.3 hour

**Is a supplement to DEALER TECHNICAL BULLETIN 92-T-119.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.