For 1990-2009 cars

### Removal Procedure

1. Remove the rear seatback.

Refer to Rear Seat Back Replacement .

2. Place the rear seatback on a clean, dry and non-abrasive surface.
3. Remove the hog rings (2).
4. Remove the rear seatback cover.

### Installation Procedure

1. Turn the pad assembly face side down on the cover.
2. Insert your hand between the cover and the foam in order to regulate the positioning of the foam pad.

Grasp the cover, positioning the foam to the inboard side of the lace skirting around the front and side facing.

3. Install the hog rings (2).
4. Install the rear seatback. Refer to Rear Seat Back Replacement .