For 1990-2009 cars

### Removal Procedure

1. Remove the lower steering column panel.
2. Remove the pushrod from the brake pedal.
3. Remove the brake pedal assembly nuts.
4. Remove the brake pedal assembly.

### Installation Procedure

1. Install the brake pedal assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the brake pedal assembly nuts.

Tighten
Tighten the brake pedal nuts to 27 N·m (20 lb ft).

3. Install the pushrod to the brake pedal.
4. Lower the steering column panel.