For 1990-2009 cars

1. Install the following onto the steering column housing assembly (1):

1.1. | The bearing adapter (4).

1.2. | The mounting plate (3).

2. Install the support mounting adapter (3).
3. Install the steering column housing assembly (2) into the support mounting adapter (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the 3 adapter screws (1).

Tighten
Tighten the screws to 5.7 (50 lb in).

5. Install the ignition switch assembly. Refer to Ignition Switch Assembly - Assemble - Off Vehicle .
6. Install the upper head component. Refer to Turn Signal Cancel Cam and Bearing Thrust Washer - Assemble - Off Vehicle .