For 1990-2009 cars

#### Tools Required

J 39579 Camshaft Sprocket Wrench

1. Remove the camshaft sprocket retaining bolts and washers. Use the J 39579 to hold the sprockets when removing the bolts.
2. Remove the camshaft sprockets. The sprockets are interchangeable, no marking is required.
3. Remove the four oil pan bolts.
4. Remove the timing chain housing to the camshaft housing bolts.
5. Remove the timing chain housing to the block bolts.
6. Remove the timing chain housing.
7. Remove the timing chain gaskets.