For 1990-2009 cars

#### Tools Required

J 34757 Snap Ring Remover and Installer

1. Remove the four case extension bolts (5).
2. Remove the case extension assembly (6) and remove the extension seal (8).
3. Leave the front differential carrier thrust washer (715) and the bearing (714) on the carrier.
4. Rotate the differential carrier until you can see the end of the output shaft.
5. Rotate the output shaft while holding the carrier, until the opening on the drive shaft snap ring is visible.
6. Use J 34757 in order to push the snap ring (512) partially off of the output shaft.
7. Remove the snap ring with needle nose pliers.

Important: Be careful not to damage the bearing on the output shaft.

8. Pull the output shaft (510) out of the transmission.