For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check or Wiper/Washer System Check
2 | Does the wiper motor operate in LO? | -- | Go to Step 3 | Go to Wipers Low Mode Inoperative, High Mode Operates
3 | Inspect the wiper motor for a bent drive pawl or excessive output shaft end play. Did you find a bent drive pawl or excessive end play? | -- | Go to Step 5 | Go to Step 4
4 | Replace the park switch. Refer to Wiper Motor Park Switch Replacement . Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --
5 | Replace the wiper motor. Refer to Windshield Wiper Motor Replacement .. Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --