For 1990-2009 cars

#### Tools Required

• | J 26958 Output Shaft Loading Tool

• | J 26958-10A Adapter Plug

• | J 38385 Output Shaft Loading Tool Adapter

1. Inspect the case extension assembly (6) for the following conditions:

• | A damaged or porous sealing surface for the case extension seal

• | A damaged or porous sealing surface for the vehicle speed sensor

• | A damaged or porous sealing surface for the right drive shaft oil seal assembly

• | Damaged bolt holes

• | A worn or damaged front differential carrier bushing (7A) or output shaft bearing assembly (7B)

• | A porous or damaged case extension housing

2. Install the differential carrier/case selective thrust washer (714) onto the differential/final drive carrier assembly (700).
3. Install the thrust bearing (715) onto the differential/final drive carrier assembly (700).
4. Affix the seal (8) onto the case extension (6).
5. Install the case extension assembly (6) onto the case (3).
6. Install only two case extension bolts (5) for later removal.

Tighten
Tighten the bolts until the extension is flush to the case.

7. Perform end play check, refer to Differential Carrier End Play Check.