For 1990-2009 cars

## Door Lock Rod Knob Replacement Pontiac

### Removal Procedure

Remove the locking rob knob (1) by pulling outward in order to disengage the knob from the locking rod. .

### Installation Procedure

Install the locking rob knob (1) by positioning the knob onto the locking rod and sliding the knob rearward.

## Door Lock Rod Knob Replacement Oldsmobile and Buick

### Removal Procedure

Remove the locking rob knob (1) by pulling outward in order to disengage the knob from the locking rod.

### Installation Procedure

Install the locking rob knob (1) by positioning the knob onto the locking rod and sliding the knob rearward.