For 1990-2009 cars

### Removal Procedure

1. Remove the upper and lower air cleaner assembly.

Notice: Do Not pry on the air cleaner assembly in order to remove the intake duct. Damage to the air cleaner may occur.

2. Remove the intake duct.

### Installation Procedure

Important: Verify full engagement of the intake duct onto the resonator neck and no contact of the air cleaner assembly to the strut tower.

1. Install the intake duct through the motor compartment front panel.
2. Install the upper and lower air cleaner assembly.