For 1990-2009 cars

## Rear Energy Absorber Replacement Oldsmobile

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Use a 4.8 mm (3/16 in) drill bit in order to drill out and remove the rivets (1).
3. Remove the energy absorber (2) from the impact bar (3).

### Installation Procedure

#### Tools Required

• | J 39312 Rivet Gun

• | J 39357 Extension

1. Install the energy absorber (2) to the impact bar (3).
2. Use the J 39312 and the J 39357 in order to install the 4.8-mm (3/16-in) pop rivets (1).
3. Install the rear fascia. Refer to Rear Bumper Fascia Replacement .

## Rear Energy Absorber Replacement Pontiac and Buick

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the push-in retainers (1).
3. Remove the energy absorber (2) from the impact bar (3).

### Installation Procedure

1. Install the energy absorber (2) to the impact bar (3).
2. Install the push-in retainers (1).
3. Install the rear fascia. Refer to Rear Bumper Fascia Replacement .