For 1990-2009 cars

### Removal Procedure

1. Position the passenger seat assembly forward to access the passenger seat buckle belt bolt.
2. Remove the front seat belt sleeve plug (3).
3. Remove the passenger seat buckle side belt bolt (2).
4. Remove the passenger seat buckle side belt.

### Installation Procedure

1. Install the passenger seat buckle side belt.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the passenger seat buckle side belt bolt (2).

Tighten
Tighten the passenger seat side belt bolt to 47 N·m (35 lb ft).

3. Install the front seat belt sleeve plug (3).