For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Center Aero Molding Nut | Fully driven, seated, not stripped
Center Molding Screw | Fully driven, seated, not stripped
Clevis Screw | 24 N·m | 18 lb in
Door Center Aero Molding Screw | Fully driven, seated, not stripped
Door Center Molding Nut | Fully driven, seated, not stripped
Door Detent to Door Nut | 5 N·m | 44 lb in
Door Detent to Hinge Pillar Bolt | 9 N·m | 80 lb in
Door Hinge to Hinge Pillar Bolt | 22 N·m | 16 lb ift
Door Inside Handle Screw | Fully driven, seated, not stripped
Door Lock Actuator TORX® Screw | 5 N·m | 40 lb in
Door Lock Cylinder Nut | 6 N·m | 53 lb in
Door Outside Handle and Lock Cylinder Bolt | 6 N·m | 53 lb in
Door Rear View Mirror Escutcheon Screw | 1 N·m | 9 lb in
Door Rear View Mirror Nut | 6 N·m | 50 lb in
Door Rear View Mirror Power Pack Screw | Fully driven, seated, not stripped
Door Speaker Screw | Fully driven, seated, not stripped
Door Trim Panel Screw | 1 N·m | 11 lb in
Door Window Assembly Nut | 11 N·m | 93 lb in
Front Door Armrest Screw | Fully driven, seated, not stripped
Front Door Window Outer Sealing Strip Screw | Fully driven, seated, not stripped
Hinge to Door Bolt | 22 N·m | 16 lb ft
Hinge to Hinge Pillar Nut | 22 N·m | 16 lb ft
Lower Door Trim Panel Nut | 2 N·m | 17 lb in
Map Pocket Nut | Fully driven, seated, not stripped
Pull Handle Screw | Fully driven, seated, not stripped
Side Roof Rail Weatherstrip Retainer Screw | Fully driven, seated, not stripped
Speaker Grille Nut | Fully driven, seated, not stripped
Upper Door Trim Panel Escutcheon Screw | Fully driven, seated, not stripped
Upper Window Run Channel Bolt | 9 N·m | 80 lb in
Window Regulator Bolt | 11 N·m | 93 lb in