For 1990-2009 cars

# RETENTION OF FROM DOOR LOCK SWITCH (RPL. DOOR LOCK BEZEL)

#### SUBJECT: RETENTION OF FRONT DOOR LOCK SWITCH - REPLACE DOOR LOCK BEZEL

#### MODELS\YEARS: 1992-1993 ACHIEVA

THIS BULLETIN HAS BEEN UPDATED TO INCLUDE THE 1992 MODEL YEAR.

#### CONDITION:

--------- Some owners of 1992-1993 Achieva models equipped with power door locks (built before VIN breakpoint PMO 1 6842) may comment on the front left and\or right-hand lock switch assemblies becoming disengaged from the bezel when the switch is pressed.

#### CAUSE:

----- Lock switch retention legs on the switch bezel are too flexible to maintain pressure against lock switch when force is applied.

#### CORRECTION:

---------- Replace door lock bezel with P\N 22588802 (RH) or 22588803 (LH) using the service procedure found in Section 10-6 of the 1993 service manual.

Parts are currently available from GMSPO.

#### PARTS INFORMATION:

Labor Operation Number: C3280 (Right) C3281 (Left) Labor Time: 0.2 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.