For 1990-2009 cars

#### Tools Required

J 33049 Camshaft Bearing Remover/Installer

1. Remove the rear camshaft cover.

Important: The camshaft bearings must not be re-used after they have been removed.

2. Use the following procedure in order to drive out the bearings:

2.1. | Select the expander assembly and driving washer.

2.2. | Assemble the J 33049 . Tighten the expander assembly snug with the camshaft bearing.

2.3. | Drive out the bearings.