For 1990-2009 cars

### Removal Procedure

1. Grasp the front center and the rear center of the dome lamp housing and squeeze the housing together until the housing releases form the base plate. Use a flat-bladed screwdriver to assist in the removal if necessary.
2. Replace the bulb if necessary.
3. Insert a flat-bladed screwdriver in the U-shaped cutout around each integral fastener in the base plate and pry the fastener downward in order to release the plate from the roof.
4. Disconnect the electrical connector.
5. Remove the base plate.

### Installation Procedure

1. Position the dome lamp base over the housing and snap the base into place.
2. Connect the electrical connector.
3. Align the retaining tabs on the cover with the holes in the base and snap the cover into place.