For 1990-2009 cars

### Removal Procedure

1. Remove the cooling system surge tank, refer to Surge Tank Replacement in Engine Cooling.
2. Disconnect the vent solenoid electrical connector.
3. Remove the vent solenoid hose clamp (2).
4. Remove the hose to the vent solenoid.
5. Remove the vent solenoid (1) from the mounting bracket.

### Installation Procedure

1. Slide the vent solenoid (1) onto the mounting bracket .
2. Lubricate the hose ends with lubricant.
3. Install the hose to the vent solenoid.
4. Tighten the vent solenoid hose clamp (2).
5. Connect the vent solenoid electrical connector.
6. Install the cooling system surge tank, refer toSurge Tank Replacement in Engine Cooling.