For 1990-2009 cars

# SERVICE MANUAL UPDATE - SPEC. REVISION (NEW ARTWORK)

#### SUBJECT: TORQUE SPECIFICATION REVISION - NEW ARTWORK FOR LOWER ENGINE MOUNT STRUT

#### MODEL/YEARS: 1992-93 ACHIEVA WITH THE 2.3L (VIN A & D) AND 3.3L (VIN N) ENGINES

This is a service manual update to Sections 6A6 and 6A7:

6A6-10, Figure 11 - Update with the illustration below. 6A7-16, Figure 16 - Update with the illustration below. 6A7-15, Figure 16 - Update with the illustration below.

The torque specification for the lower engine mount strut has been revised. Refer to the illustration below. The specification that has changed has a box around it.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.