For 1990-2009 cars

Checks | Causes
--- | ---
Key Cannot be Removed in the OFF Position | Inspect the steering column lock system for the following conditions:

• | A damaged ignition switch assembly

• | A bent or twisted ignition key

• | A damaged lock cylinder assembly

• | An improper park lock cable adjustment

• | An improper shift control cable adjustment

• | A damaged electric park lock solenoid