For 1990-2009 cars

### Removal Procedure

1. Remove the recliner cover screws.
2. Remove the reclining cover.
3. Remove the cable casing end cap from the casing retainer.
4. Remove the cable (2) from the lock bar (3).
5. Remove the cable end cap from the retainer.
6. Remove the cable (2) from the actuating lever (1).

### Installation Procedure

1. Install the cable (2) to the actuating lever (1).
2. Install the cable end cap to the retainer.
3. Install the cable (2) to the lock bar (3).
4. Install the cable end cap to the casing retainer.
5. Install the recliner cover.
6. Install the recliner cover screws.