For 1990-2009 cars

### Removal Procedure

1. Open the hood (2).
2. Remove the hood latch striker retaining bolts (3).
3. Remove the hood latch striker (1).

### Installation Procedure

1. Install the hood latch striker (1).
2. Install the hood latch striker retaining bolts (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Align the hood primary latch striker to the hood primary and secondary latch.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

4. Close the hood.