For 1990-2009 cars

## Door Handle Bezel Replacement Pontiac

### Removal Procedure

1. Remove the screw (1) from the bezel.
2. Pull the front of the bezel out of the door trim panel (2).
3. Lift the door handle and remove the bezel.

### Installation Procedure

1. Push the bezel into the trim panel, making sure the rear tabs engage and press until fully seated.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the door handle bezel screw (1).

Tighten
Tighten the front/rear door handle bezel screw to 3 N·m (27 lb in).