For 1990-2009 cars

### Removal Procedure

Important: There is no service interval for fuel filter replacement. Only replace the fuel filter if it is restricted. Inspect the fuel tank internally and clean the fuel tank if you find a restricted fuel filter.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Disconnect the fuel filter fitting using a back-up wrench.
4. Disconnect the quick connect fitting from the fuel filter. Refer to Plastic Collar Quick Connect Fitting Service .
5. Remove the fuel filter.

### Installation Procedure

1. Remove the protective caps from the new fuel filter.
2. Install the fuel filter (2) in the same position as the old fuel filter.
3. Connect the fuel filter quick connect fitting. Refer to Plastic Collar Quick Connect Fitting Service .

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Connect the fuel filter fitting (3) using a back-up wrench.

Tighten
Tighten the fuel filter fitting to 27 N·m (20 lb ft).

5. Lower the vehicle.
6. Connect the negative battery cable.
7. Inspect for fuel leaks using the following procedure:

7.1. | Turn ON the ignition, with the engine OFF for 2 seconds.

7.2. | Turn OFF the ignition for 10 seconds.

7.3. | Turn ON the ignition, with the engine OFF.

7.4. | Inspect for fuel leaks.