For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Hydraulic Brake Diagnostic System Check? | -- | Go to Step 2 | Go to Hydraulic Brake Diagnostic System Check
2 | Inspect the front suspension for loose or missing components. Did you find any loose or missing components? | -- | Go to Step 3 | Go to Step 4
3 | Tighten, repair or replace missing the components as necessary. Refer to Fastener Tightening Specifications in Front Suspension. Did you complete the repair? | - | Go to Hydraulic Brake Diagnostic System Check | --
4 | Inspect the disc brake pads and brake shoe linings for the following conditions:

• | Excessive wear

• | Uneven wear

• | Abuse

• | Glazing

• | Contaminated lining material

• | Incorrect lining material

Did you find a condition?

--

Go to Step 5

Go to Step 6

5 | Replace the brake linings. Refer to the following procedures:

• | Front Disc Brake Pads Replacement in Disc Brakes

• | Rear Disc Brake Pads Replacement in Disc Brakes

• | Brake Shoe Replacement in Drum Brakes

Did you complete the repair?

--

Go to Hydraulic Brake Diagnostic System Check

--

6 | Inspect the wheel assemblies for out of balance condition. Are any of the wheel assemblies out of balance? | -- | Go to Step 7 | Go to Step 8
7 | Balance the wheel assembly. Refer to Tire and Wheel Balancing in Vibration Diagnosis and Correction. Did you complete the repair? | -- | Go to Hydraulic Brake Diagnostic System Check | --
8 | Verify proper brake system operation. Does the original condition still exist? | -- | Go to Hydraulic Brake Diagnostic System Check | System OK