For 1990-2009 cars
Engine Controls Components
Engine Controls Schematics
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The stepper motor cruise control module sends the cruise status input to the PCM to indicate when cruise control is engaged. The PCM monitors the cruise status signal while commanding cruise to be disengaged by grounding the cruise inhibit circuit. Any of the following conditions may cause the PCM to inhibit cruise control operation:

• | Engine not running long enough for cruise control operation.

• | Transaxle range inputs indicate park, neutral, low, or reverse gear selected.

• | Engine speed is too high or too low.

• | Vehicle speed is too high or too low.

• | ABS system is active for longer than 2 seconds.

• | Vehicle acceleration or deceleration rate is too high.

### Conditions for Setting the DTC

• | The PCM is commanding the SMCC module to not allow cruise control operation (Cruise Inhibit circuit grounded).

• | The Cruise Status input to the PCM indicates that cruise control is still active.

• | Above conditions for longer than 1 second.

### Action Taken When the DTC Sets

The PCM stores conditions which were present when the DTC set as Failure Records only. This information will not be stored as Freeze Frame Records.

### Conditions for Clearing the MIL/DTC

• | The DTC becomes history when the conditions for setting the DTC are no longer present.

• | The history DTC clears after 40 malfunction free warm-up cycles.

• | The PCM receives a clear code command from the scan tool.

### Diagnostic Aids

Check for the following conditions:

• | Poor connection at PCM. Inspect harness connectors for backed out terminals, improper mating, broken locks, improperly formed or damaged terminals, and poor terminal to wire connection.

• | Damaged harness. Inspect the wiring harness for damage. If the harness appears to be OK, observe the Cruise Status display on the scan tool while moving connectors and wiring harnesses related to the Stepper Motor Cruise Control module. A change in the display will indicate the location of the fault.

If DTC P1554 cannot be duplicated, the information included in the Failure records data can be useful in determining how many ignition cycles have passed since the DTC was last set.

### Test Description

The numbers below refer to the step numbers on the Diagnostic Table.

1. This vehicle is equipped with a PCM which utilizes an Electrically Erasable Programmable Read Only Memory (EEPROM). When the PCM is being replaced, the new PCM must be programmed.

#### DTC P1554 - Cruise Control Status Circuit

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain ON Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to the Powertrain On Board Diagnostic (OBD) System Check
2 | Is DTC P1662 also set? | -- | Go to DTC P1662 Cruise Control Inhibit Output Circuit | Go to Step 3
3 |

1. Turn OFF the ignition switch.
2. Disconnect the cruise control module.
3. Turn ON the ignition switch.
4. Using a J 39200 digital multimeter (DMM), measure voltage between the Cruise Engaged Input circuit at the cruise control module harness connector and ground.

Is voltage greater than the specified value?

7.0V

Go to Step 4

Go to Step 5

4 |

1. Turn OFF the ignition switch.
2. Reconnect the cruise control module.
3. Disconnect the PCM.
4. Turn ON the ignition switch.
5. Probe the Cruise Engaged Input circuit at the PCM harness connector with a test lamp to battery positive voltage.

Is the test lamp ON?

--

Go to Step 6

Go to Step 7

5 |

1. Turn OFF the ignition switch.
2. Disconnect the PCM.
3. Probe the Cruise Engaged Input circuit at the PCM harness connector with a test lamp to battery positive voltage.

Is the test lamp ON?

--

Go to Step 8

Go to Step 7

6 | Replace the cruise control module. Refer to Cruise Control Module Replacement Is the action complete? | -- | Go to Step 9 | --
7 | Important: The replacement PCM must be programmed. Refer to Powertrain Control Module Replacement/Programming . Replace the PCM. Is the action complete? | -- | Go to Step 9 | --
8 | Locate and repair short to ground in the Cruise Engaged Input circuit. Refer to Wiring Repairs . Is the action complete? | -- | Go to Step 9 | --
9 |

1. Clear DTC P1554.
2. Start the engine and observe DTCs.

Did DTC P1554 set?

--

Go to Step 2

System OK